Appendix F – Log Scaling Lengths and Rules for Butt Logs

The following reference will be used for the log scaling portion of the Timber measurement Skillset, “National Forest Log Scaling Handbook”   https://fs.fed.us/im/directives/fsh/2409.11/2409.11-NF%20LOGSCALING%20HDBK.pdf

Scaling Rules:
	When logs are measured for length, they must be in even 2 foot increments that include 6 inches of trim if they do not have the needed 6 inches then they will be scaled to the next shorter 2 foot increment.  For example, a 16' 8" log would be scaled as a 16' log; a 16' 2" log would be scaled as a 14" log.  Two segment logs must have a minimum of 1 foot of trim or 6 inches for each segment.

Given logs should be no less than 12'6" to be scaled as a 12' log to accommodate the Spencer Scaling Tape

Rules for scaling butt logs:
	20’ and under, no taper
	22’ - 26’, 1” taper per segment, 2” total taper.
	28’ - 40’, 2” taper per segment, 4” total taper

